(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(title_block
		(title "left_pcb")
		(date "2025-08-10")
		(rev "v0.2")
		(company "Happily-Coding")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.05)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "col1_row4")
	(net 2 "C1")
	(net 3 "GND")
	(net 4 "col1_row3")
	(net 5 "col1_row2")
	(net 6 "col1_row1")
	(net 7 "col2_row5")
	(net 8 "C2")
	(net 9 "col2_row4")
	(net 10 "col2_row3")
	(net 11 "col2_row2")
	(net 12 "col2_row1")
	(net 13 "col3_row5")
	(net 14 "C3")
	(net 15 "col3_row4")
	(net 16 "col3_row3")
	(net 17 "col3_row2")
	(net 18 "col3_row1")
	(net 19 "col4_row4")
	(net 20 "C4")
	(net 21 "col4_row3")
	(net 22 "col4_row2")
	(net 23 "col4_row1")
	(net 24 "col5_row4")
	(net 25 "C5")
	(net 26 "col5_row3")
	(net 27 "col5_row2")
	(net 28 "col5_row1")
	(net 29 "col6_row4")
	(net 30 "C6")
	(net 31 "col6_row3")
	(net 32 "col6_row2")
	(net 33 "col6_row1")
	(net 34 "col7_row4")
	(net 35 "C7")
	(net 36 "col7_row3")
	(net 37 "col7_row2")
	(net 38 "col1_thumb_row_1")
	(net 39 "col2_thumb_row_1")
	(net 40 "col3_thumb_row_1")
	(net 41 "R4")
	(net 42 "R3")
	(net 43 "R2")
	(net 44 "R1")
	(net 45 "R5")
	(net 46 "RAW")
	(net 47 "RST")
	(net 48 "VCC")
	(net 49 "P10")
	(net 50 "DPC")
	(net 51 "DPD")
	(net 52 "DPE")
	(net 53 "R7")
	(net 54 "R6")
	(net 55 "P101")
	(net 56 "P102")
	(net 57 "P107")
	(net 58 "BAT_P")
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 61.25 82.03 -90)
		(property "Reference" "D13"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "col3_row2")
		)
	)
	(footprint "ceoloide:mcu_nice_nano"
		(layer "F.Cu")
		(at 81.75 45.77 90)
		(property "Reference" "MCU1"
			(at 0 -15 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "R5"
			(at 4.47 15.24 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "VCC"
			(at -4.47 -5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "C1"
			(at -4.47 -2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 90)
			(layer "B.SilkS")
		)
		(fp_text user "C7"
			(at -4.47 12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "C1"
			(at -4.47 -2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at -4.47 -5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 15.24 90)
			(layer "F.SilkS")
		)
		(fp_text user "C7"
			(at -4.47 12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 7.62 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "DPC")
		)
		(pad "2" thru_hole circle
			(at 7.62 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "DPD")
		)
		(pad "3" thru_hole circle
			(at 7.62 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "4" thru_hole circle
			(at 7.62 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole circle
			(at 7.62 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "DPE")
		)
		(pad "6" thru_hole circle
			(at 7.62 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "R2")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "R3")
		)
		(pad "8" thru_hole circle
			(at 7.62 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "R5")
		)
		(pad "9" thru_hole circle
			(at 7.62 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "R4")
		)
		(pad "10" thru_hole circle
			(at 7.62 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "R7")
		)
		(pad "11" thru_hole circle
			(at 7.62 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "R6")
		)
		(pad "12" thru_hole circle
			(at 7.62 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "R5")
		)
		(pad "13" thru_hole circle
			(at -7.62 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "P10")
		)
		(pad "14" thru_hole circle
			(at -7.62 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "C7")
		)
		(pad "15" thru_hole circle
			(at -7.62 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "C6")
		)
		(pad "16" thru_hole circle
			(at -7.62 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "C5")
		)
		(pad "17" thru_hole circle
			(at -7.62 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "C4")
		)
		(pad "18" thru_hole circle
			(at -7.62 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "C3")
		)
		(pad "19" thru_hole circle
			(at -7.62 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "C2")
		)
		(pad "20" thru_hole circle
			(at -7.62 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "C1")
		)
		(pad "21" thru_hole circle
			(at -7.62 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "VCC")
		)
		(pad "22" thru_hole circle
			(at -7.62 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "RST")
		)
		(pad "23" thru_hole circle
			(at -7.62 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "24" thru_hole circle
			(at -7.62 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "RAW")
		)
		(pad "25" thru_hole circle
			(at 5.08 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "P101")
		)
		(pad "26" thru_hole circle
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "P102")
		)
		(pad "27" thru_hole circle
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "P107")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 112.25 126.23 -90)
		(property "Reference" "D23"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "col6_row4")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 101.4082 141.907 -100)
		(property "Reference" "D30"
			(at 0 0 -100)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -100)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -100)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -100)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -100)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0.000001 260)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "R5")
		)
		(pad "2" smd rect
			(at 1.65 -0.000001 260)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "col1_thumb_row_1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 112.25 75.23 -90)
		(property "Reference" "D26"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "col6_row1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 112.25 92.23 -90)
		(property "Reference" "D25"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "col6_row2")
		)
	)
	(footprint "ceoloide:mounting_hole_npth"
		(layer "F.Cu")
		(at 29.05 138.95)
		(property "Reference" "MH2"
			(at 0 2.55 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 95.25 122.83 -90)
		(property "Reference" "D19"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "col5_row4")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 112.25 109.23 -90)
		(property "Reference" "D24"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "col6_row3")
		)
	)
	(footprint "ceoloide:battery_connector_jst_ph_2"
		(layer "F.Cu")
		(at 114 55.77 -90)
		(property "Reference" "JST1"
			(at 0 4.8 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -1 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2)
			(net 3 "GND")
		)
		(pad "2" thru_hole oval
			(at 1 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "BAT_P")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 44.25 76.25 -90)
		(property "Reference" "D9"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "col2_row1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 44.25 110.25 -90)
		(property "Reference" "D7"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "col2_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 44.25 93.25 -90)
		(property "Reference" "D8"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "col2_row2")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 114.5 -90)
		(property "Reference" "D2"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "col1_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 44.25 127.25 -90)
		(property "Reference" "D6"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "col2_row4")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 120.5808 145.8308 -115)
		(property "Reference" "D31"
			(at 0 0 -115)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -115)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -115)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 245)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 245)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "col2_thumb_row_1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 61.25 65.03 -90)
		(property "Reference" "D14"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "col3_row1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 95.25 71.83 -90)
		(property "Reference" "D22"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "col5_row1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 78.25 120.28 -90)
		(property "Reference" "D15"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "col4_row4")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 78.25 86.28 -90)
		(property "Reference" "D17"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "col4_row2")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 61.25 133.03 -90)
		(property "Reference" "D10"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "col3_row5")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 131.5 -90)
		(property "Reference" "D1"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "col1_row4")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 78.25 103.28 -90)
		(property "Reference" "D16"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "col4_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 95.25 88.83 -90)
		(property "Reference" "D21"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "col5_row2")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 129.25 88.83 -90)
		(property "Reference" "D29"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "col7_row2")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 80.5 -90)
		(property "Reference" "D4"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "col1_row1")
		)
	)
	(footprint "ceoloide:mounting_hole_npth"
		(layer "F.Cu")
		(at 114.05 82.68)
		(property "Reference" "MH3"
			(at 0 2.55 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 129.25 105.83 -90)
		(property "Reference" "D28"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "col7_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 61.25 116.03 -90)
		(property "Reference" "D11"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "col3_row4")
		)
	)
	(footprint "ceoloide:mounting_hole_npth"
		(layer "F.Cu")
		(at 29.05 87.95)
		(property "Reference" "MH1"
			(at 0 2.55 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 136.7316 153.4761 -120)
		(property "Reference" "D32"
			(at 0 0 -120)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -120)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -120)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -120)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -120)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 240)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 240)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "col3_thumb_row_1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 78.25 69.28 -90)
		(property "Reference" "D18"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "col4_row1")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 95.25 105.83 -90)
		(property "Reference" "D20"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "col5_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 129.25 122.83 -90)
		(property "Reference" "D27"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "col7_row4")
		)
	)
	(footprint "ceoloide:mounting_hole_npth"
		(layer "F.Cu")
		(at 114.05 133.68)
		(property "Reference" "MH4"
			(at 0 2.55 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ceoloide:mounting_hole_npth"
		(layer "F.Cu")
		(at 119.0636 153.3435 -25)
		(property "Reference" "MH5"
			(at 0 2.55 -25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -25)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0 335)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 61.25 99.03 -90)
		(property "Reference" "D12"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "col3_row3")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 44.25 144.25 -90)
		(property "Reference" "D5"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "col2_row5")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 97.5 -90)
		(property "Reference" "D3"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "col1_row2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 86 70.78)
		(property "Reference" "S18"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "col4_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 69 83.53)
		(property "Reference" "S13"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "col3_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 142.6933 158.6502 -30)
		(property "Reference" "S32"
			(at 0 8.8 -30)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -30)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -30)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0 330)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95 330)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0 330)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 165)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0 330)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95 330)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "col3_thumb_row_1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75 330)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 120 76.73)
		(property "Reference" "S26"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "col6_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 69 134.53)
		(property "Reference" "S10"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "col3_row5")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 52 111.75)
		(property "Reference" "S7"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "col2_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 103 107.33)
		(property "Reference" "S20"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "col5_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 120 127.73)
		(property "Reference" "S23"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 29 "col6_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 137 90.33)
		(property "Reference" "S29"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 37 "col7_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 137 107.33)
		(property "Reference" "S28"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 36 "col7_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 52 77.75)
		(property "Reference" "S9"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "col2_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 126.9707 150.4655 -25)
		(property "Reference" "S31"
			(at 0 8.800001 -25)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -25)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0 335)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95 335)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0 335)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 170)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0 335)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95 335)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "col2_thumb_row_1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75 335)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 86 104.78)
		(property "Reference" "S16"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "col4_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 86 121.78)
		(property "Reference" "S15"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "col4_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 137 124.33)
		(property "Reference" "S27"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 34 "col7_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 116)
		(property "Reference" "S2"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "col1_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 69 117.53)
		(property "Reference" "S11"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "col3_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 103 90.33)
		(property "Reference" "S21"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "col5_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 52 145.75)
		(property "Reference" "S5"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "col2_row5")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "C2")
		)
	)
	(footprint "ceoloide:power_switch_smd_side"
		(layer "B.Cu")
		(at 108 37.77 90)
		(property "Reference" "PWR1"
			(at -3.6 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "PWR1"
			(at -3.5 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "ON"
			(at 0 -5 90)
			(layer "B.SilkS")
		)
		(fp_text user "OFF"
			(at 0 5 90)
			(layer "B.SilkS")
		)
		(pad "" smd rect
			(at -1.085 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at -1.085 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 -1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 1.125 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at 1.125 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "1" smd rect
			(at -1.735 -2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "BAT_P")
		)
		(pad "2" smd rect
			(at -1.735 0.75)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "RAW")
		)
		(pad "3" smd rect
			(at -1.735 2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 103 73.33)
		(property "Reference" "S22"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "col5_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 69 66.53)
		(property "Reference" "S14"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "col3_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 82)
		(property "Reference" "S4"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "col1_row1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 99)
		(property "Reference" "S3"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "col1_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 120 93.73)
		(property "Reference" "S25"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 32 "col6_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 69 100.53)
		(property "Reference" "S12"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "col3_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 52 128.75)
		(property "Reference" "S6"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "col2_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "C2")
		)
	)
	(footprint "ceoloide:reset_switch_smd_side"
		(layer "B.Cu")
		(at 112 45.77 -90)
		(property "Reference" "RST1"
			(at 0 0 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -2.625 -0.85 90)
			(size 1.55 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "GND")
		)
		(pad "2" smd rect
			(at -2.625 0.85 90)
			(size 1.55 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "RST")
		)
		(pad "3" smd rect
			(at 2.625 -0.85 90)
			(size 1.55 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "GND")
		)
		(pad "4" smd rect
			(at 2.625 0.85 90)
			(size 1.55 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "RST")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 52 94.75)
		(property "Reference" "S8"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "col2_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 86 87.78)
		(property "Reference" "S17"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "col4_row2")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 103 124.33)
		(property "Reference" "S19"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "col5_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 133)
		(property "Reference" "S1"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "col1_row4")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 120 110.73)
		(property "Reference" "S24"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 31 "col6_row3")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 108.78 144.73 -10)
		(property "Reference" "S30"
			(at 0 8.8 -10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -10)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -10)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -10)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -10)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0 350)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95 350)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0 350)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 185)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0 350)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95 350)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "col1_thumb_row_1")
		)
		(pad "2" smd rect
			(at 8.275 -3.75 350)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "C5")
		)
	)
	(gr_line
		(start 63 153.75)
		(end 63 145.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 27 144)
		(end 41 144)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 147.95804 115.83)
		(mid 147.989493 116.079121)
		(end 148 116.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 95 135.33)
		(mid 93.044239 134.604863)
		(end 92.033942 132.78)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131 135.73)
		(mid 130.12132 137.85132)
		(end 128 138.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131 135.73)
		(end 131 135.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.267781 135.33)
		(end 96.557929 150.698332)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.265101 164.176449)
		(mid 130.098227 164.072671)
		(end 129.938504 163.958193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128 65.73)
		(end 118 65.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131 79.33)
		(end 131 68.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.219584 171.078373)
		(end 156.219584 157.221967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.75 55.53)
		(end 61 55.53)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24.04196 124.5)
		(mid 24.010507 124.250879)
		(end 24 124)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41 69.75)
		(mid 41.87868 67.62868)
		(end 44 66.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41 71)
		(end 27 71)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148.219584 171.078373)
		(mid 146.397965 172.476168)
		(end 144.121508 172.176449)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104 62.33)
		(end 96.966058 62.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 44 156.75)
		(mid 41.87868 155.87132)
		(end 41 153.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118 65.73)
		(end 118 53.77)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41 69.75)
		(end 41 71)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.832053 138.73)
		(end 128 138.73)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.75 31.27)
		(mid 113.87132 32.14868)
		(end 114.75 34.27)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24 108)
		(mid 24.010509 107.749121)
		(end 24.04196 107.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 63 153.75)
		(mid 62.12132 155.87132)
		(end 60 156.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41 144)
		(end 41 153.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24 91)
		(mid 24.010509 90.749121)
		(end 24.04196 90.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148 132.33)
		(end 148 116.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.071465 157.053954)
		(mid 114.994228 157.016586)
		(end 114.918093 156.977021)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148 115.33)
		(end 148 99.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24.04196 90.5)
		(mid 24.010507 90.250879)
		(end 24 90)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148 115.33)
		(mid 147.989491 115.580879)
		(end 147.95804 115.83)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 80 142.53)
		(mid 79.12132 144.65132)
		(end 77 145.53)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24 125)
		(mid 24.010509 124.749121)
		(end 24.04196 124.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63 145.53)
		(end 77 145.53)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24 74)
		(mid 24.87868 71.87868)
		(end 27 71)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.75 50.77)
		(end 114.75 34.27)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148 98.33)
		(mid 147.989491 98.580879)
		(end 147.95804 98.83)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.121508 153.123891)
		(end 141.265102 145.123891)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.75 34.27)
		(mid 65.62868 32.14868)
		(end 67.75 31.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 44 156.75)
		(end 60 156.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24.04196 107.5)
		(mid 24.010507 107.250879)
		(end 24 107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.071465 157.053954)
		(end 129.572389 163.815846)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 145 79.33)
		(mid 147.12132 80.20868)
		(end 148 82.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 24 125)
		(end 24 141)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 27 144)
		(mid 24.87868 143.12132)
		(end 24 141)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115 50.77)
		(end 114.75 50.77)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.75 31.27)
		(end 67.75 31.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 24 74)
		(end 24 90)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.643137 60.27)
		(end 104 60.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 79.33)
		(end 131 79.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58 58.53)
		(end 58 66.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131 135.33)
		(end 145 135.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148 98.33)
		(end 148 82.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.938504 163.958193)
		(mid 129.753115 163.893016)
		(end 129.572389 163.815846)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 128 65.73)
		(mid 130.12132 66.60868)
		(end 131 68.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80 132.78)
		(end 92.033942 132.78)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104 60.27)
		(end 104 62.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.991408 154.1737)
		(end 114.748332 156.952071)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115 50.77)
		(mid 117.12132 51.64868)
		(end 118 53.77)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58 58.53)
		(mid 58.87868 56.40868)
		(end 61 55.53)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.869991 143.877075)
		(mid 139.458998 144.239725)
		(end 139.949302 144.727627)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148 132.33)
		(mid 147.12132 134.45132)
		(end 145 135.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 95.643137 60.27)
		(mid 96.524296 61.158911)
		(end 96.966058 62.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 147.95804 98.83)
		(mid 147.989493 99.079121)
		(end 148 99.33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58 66.75)
		(end 44 66.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80 142.53)
		(end 80 132.78)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.869991 143.877075)
		(end 127.832053 138.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 24 91)
		(end 24 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.918093 156.977022)
		(mid 114.833034 156.965761)
		(end 114.748332 156.952071)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.991408 154.1737)
		(mid 97.054937 152.939994)
		(end 96.557929 150.698332)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 24 108)
		(end 24 124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.265101 164.176449)
		(end 144.121508 172.176449)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155.121508 153.12389)
		(mid 156.519304 154.945514)
		(end 156.219584 157.221967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.75 34.27)
		(end 64.75 55.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95 135.33)
		(end 99.267781 135.33)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 139.949302 144.727627)
		(mid 140.630197 144.849404)
		(end 141.265102 145.123891)
		(layer "Edge.Cuts")
	)
)
